Frey Test Code

*Constant Transmit Parameters*

* Control Parameter

Selection between ON/OFF for the continuous transmit

* Band Selection

Selection between transmit bands: B2, B4, B12, B13

* Channels

Selection of High, Middle, or Low channel of selected transmit band.

B2 – High, Mid, Low (EARFCN – 18600, 18900, 19199)

B4 – High, Mid, Low (EARFCN – 19950, 20175, 20399)

B12 – High, Mid, Low (EARFCN – 23010, 23095, 23179)

B13 – High, Mid, Low (EARFCN – 23180, 23230, 23279)

* Power

Selection between the following output power levels:

-10, 0, 10, 23dBm

*Defaults*

If a default setting is needed; when the VPro is first turned on the following default should be used:

Control –> Off

Band –> B2

Channel –> Low

Power –> -10dBm